- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Problem on tray detector (1533)

Error content | There is a boot program but no application program in the detector.
Detail | Separated by sub-error No. 0000: No application program exists. A boot program started. 0001: A boot program has started while between pin 2 and 3 of Jumper SW (JP2) in the detector board is short circuit.
Solution | [OK] button => Operate without the tray detector. (Operate with registered trays.)
Action by user |
Action by service representative | Sub-error No.: 0000 A download of the detector application is required. Sub-error No.: 0001 Perform switching by short circuiting between pin 1 and 2 for the short circuit socket between pin 2 and 3 of the jumper SW (JP2) on the detector board.
Related part | Detector board [A221]
Remarks |