Error Number | Error Content
Normal | P Type | JW Type
401 |  |  | Wrapper is not connected
402 |  |  | No response from wrapper
403 |  |  | Problem caused on wrapper
406 |  |  | Wrapper detected temporary blackout
407 |  |  | Temporary blackout on console
409 |  |  | No response from wrapper
410 |  |  | Lift motor is abnormal
411 |  |  | Motor for film feed is abnormal
412 |  |  | Motor for film change is abnormal
413 |  |  | Film driving motor is abnormal
415 |  |  | Motor for back squeeze plate is abnormal
416 |  |  | Motor for R/L squeeze is abnormal
417 |  |  | Outfeed pusher motor is abnormal
418 |  |  | Feeder motor is abnormal
419 |  |  | Motor front feeder move is abnormal
420 |  |  | Motor rear feeder move is abnormal
421 |  |  | Feed bar motor is abnormal
422 |  |  | Centering motor is abnormal
423 |  |  | Lift change is abnormal
424 |  |  | Outfeed change motor is abnormal
426 |  |  | Film heater has problem
434 |  |  | Something is stuck underneath of lift
435 |  |  | Motor voltage is abnormal
440 |  |  | Emergency stop has been pushed
441 |  |  | Film remove cover is open
444 |  |  | Film exchange cover is open
445 |  |  | Front cover is opened
447 |  |  | Infeed conveyor is out
448 |  |  | Do not put your hands into the machine
449 |  |  | Do not put your hands into the machine
|  | 451 | Under labeller unit is out
|  | 452 | Roller for under labeller is out
459 |  |  | Machine is returning to standby position (0000)
459 |  |  | Machine is returning to standby position (9999)
460 |  |  | Product was not feeded
461 |  |  | Film over error for the upper
465 |  |  | Film feeding error for the upper
466 |  |  | Film feeding error for the lower
467 |  |  | Film loading was failed on the upper
|  | 468 | It missed to print underlabeller
|  | 469 | Stock part is not ready
470 |  |  | There is problem on wrapping controller
471 |  |  | There is problem on wrapping controller
472 |  |  | There is problem on wrapping controller
473 |  |  | There is problem on seal heater
474 |  |  | There is problem on seal heater
475 |  |  | Wrong selection for big/small lift
476 |  |  | Wrong tray against programmed tray
477 |  |  | Feeder bar is not original position
478 |  |  | Insert plate is not set for the upper
479 |  |  | Insert plate is not set for the lower
480 |  |  | Film is remaining (0001)
480 |  |  | Film is remaining (0100)
480 |  |  | Film is remaining (0101)
481 |  |  | Cutter is not back to original position
482 |  |  | Insert plate is not back to original position
483 |  |  | Sensor for the back side of feeder is abnormal
484 |  |  | Heater safety guard is up
485 |  |  | Auxiliary for magnetic contact is abnormal
486 |  |  | Product is on the lift
490 |  |  | Film loading for the upper (0000)
490 |  |  | Film loading for the lower (0001)
491 |  |  | Film loading for the upper is completed (0000)
491 |  |  | Film loading for the lower is completed (0001)
492 |  |  | Film removal is completed (0001)
492 |  |  | Film removal is completed (0002)
494 |  |  | Problem on wrapping part
495 |  |  | Sum value for receiving is abnormal
496 |  |  | Writing for flash ROM is busy
497 |  |  | Failed in writing in flash ROM
498 |  |  | Problem on wrapping part
593 |  |  | Preparing film set (0000)
593 |  |  | Preparing film set (0001)
597 |  |  | Film loading instructions (0000)
597 |  |  | Film loading instructions (0001)