< Outfeed change motor is abnormal (424)

Error content | Outfeed change motor error.
Detail | An error occurred in the stock conveyor attached to the wrapper. Outfeed change motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A300] 嘇 Driving motor for outfeed conveyor [M07]
Remarks |