< Insert plate is not set for the lower (479)

Error content | Insert plate is not set for the lower.
Detail | Film exchange cover is closed, but lower film insert open/close is open.
Solution | Press the [RETURN] button after setting the insert plate.
Action by user |
Action by service representative |
Related part | <If the error occurs even after the insert open/close is closed> 嘆 P-1105 [A300] 嘇 Lower film inserts open/close [B305]
Remarks |