< Problem on wrapping part (498)

Error content | Wrapper system error.
Detail | A malfunction occurred in the wrapper program. Sub-error meanings are as follows: 001X to 003X: CAN communications are not synchronized. 0012: For a wrapping request, only child (A100) received a command / For sending hold instruction, no response was received. 0013: For a discharge request, only child (A100) received a command / For sending hold instruction, no response was received. 0017: For a wrapping request, only child (A100) received a command / For sending hold instruction, different answer from sending was returned. 0018: For a discharge request, only child (A100) received a command / For sending hold instruction, different answer from sending was returned. 0022: For a wrapping request, only child(A300) received a command / For sending hold instruction, no response was received. 0023: For a discharge request, only child(A300) received a command / For sending hold instruction, no response was received. 0027: For a wrapping request, only child(A300) received a command / For sending hold instruction, different answer from sending was returned. 0028: For a discharge request, only child(A300) received a command / For sending hold instruction, different answer from sending was returned. 0032: For a wrapping request, both of child(A100) and child(A300) received a command / For sending hold instruction, no response was received. 0033: For a discharge request, both of child(A100) and child(A300) received a command / For sending hold instruction, no response was received. 0037: For a wrapping request, both of child(A100) and child(A300) received a command / For sending hold instruction, different answer from sending was returned. 0038: For a discharge request, both of child(A100) and child(A300) received a command / For sending hold instruction, different answer from sending was returned. 1014: Operation was not completed after the grip operation protection timer run out. 1017: Operation was not completed after the cutter operation protection timer run out.
Solution | Restore power
Action by user |
Action by service representative |
Related part |
Remarks |