- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Abnormal for sensor (POP label) (616-2040)

Error content | Abnormal for applicator sensor.
Detail | A sensor that does not have light blocked is blocked from light. Sub-error meaning is as follows: 2040: X axis
Solution | Press [RETURN] button.
Action by user |
Action by service representative |
Related part | (1) X-axis origin point of POP printer [B407] (2) Suction position of POP printer [B406]
Remarks |