- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Cutter error (1069-0000)

Error content | Operation error of the under labeller cutter.
Detail | The cutter did not go back to the original position in the cutting operation after issuing the label.
Solution | After confirming that the label is not jammed, perform the unloaded feed.
Action by user |
Action by service representative |
Related part |
Remarks |