- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Thermal head for under labeller is up (1016-0002)

Error content | Thermal head for the under labeller is up.
Detail | The thermal head was up when printing starts. Displaying when closing the front cover or setting the under labeller unit.
Solution | Pull the under labeller unit out, press [RETURN] button after setting the thermal head.
Action by user |
Action by service representative |
Related part |
Remarks |