< Thermal head is worn out for printer 1 (715-0001, 815-0001)

Error content | Thermal head is worn out for printer 1.
Detail | Affected content is separated by sub-error No. 0001: The portion that as run out has no effect on printing.
Solution | [EXEC] button, [STOP] button [EXEC]: Head check is performed to the next product. [STOP]丟 Head check is not performed to the next product.
Action by user |
Action by service representative |
Related part |
Remarks | 乬Printer No.1乭 changes depending on error No.