< It could not suck label (609)

Error content | Applicator failed in label application.
Detail | Sub-error meanings are as follows: 0000: Applicator failed in labeled absorption.
Solution | Use either (1) or (2) to clear the error. 嘆 [RETURN] button 嘇 [PLU] button
Action by user | Clean up the label presence sensor.
Action by service representative | Clean up the label presence sensor. Adjust the issue position by printing adjustment. Adjust the suction position on the printer adjustment screen.
Related part | 嘆 P-1105 [A100] 嘇 P-1006 [A101] 嘊 Label presence [B116] 嘋 Label suction fan [M107]
Remarks |