- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Roller for under labeller is out (0371)

Error content | Roller for under labeller is out.
Detail | Operate again after pulling the under labeller unit out.
Solution | Set the under labeller roller.
Action by user |
Action by service representative | Check the electromagnetic contactor displaying error when the under labeller unit is set.
Related part |
Remarks |