- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Insert plate is not back to original position (482)

Error content | The insertion plate is not returned to the original position.
Detail | The cutter does not work when trying to start the cutter operation because the insertion plate is not returned to the original position. The sub-error has the following meanings: 0000: The insertion plate is not returned to the original position when cutting at the upper film feeder. 0001: The insertion plate is not returned to the original position when cutting at the lower film feeder. 0006: The film-feeding insertion plate is not returned to the original position during resetting operation. 0007: The insertion plate is not returned to the original position during loading.
Solution | Press the [RETURN] button after confirming the insertion plate.
User’s action |
Service person’s action | When “0498-0027” is also displayed, it is the cause.
Related part | ① P-1105 [A300] (lower left) ② Insertion origin [B301] (rear side, upper left)
Remarks |