< No response from applicator (650)

Error content | No response from applicator except for power-on notification.
Detail | 丒 Communication wasn't achieved between the console and the applicator. 丒 Communication phase number is in the sub-error. 丒 Communication errors after power ON result in this error.
Solution | [STOP]=> Cut communication with the applicator. Operate without the applicator. [REEXEC] => Check connection with the applicator. The error is cleared if connection is confirmed.
Action by user |
Action by service representative |
Related part |
Remarks | Operation without the applicator is possible after pressing the [STOP] button.