- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Abnormal for sensor (616)

Error content | Abnormal for sensor.
Detail | A sensor that does not have light blocked is blocked from light. Sub-error meanings are as follows: 0000: X axis
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① X-axis origin point [B108] ① Printer No.1 position [B109] ② Printer No.2 position [B110]
Remarks |