- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■Underlabeller Error (01040-0002)

Error content | Check the label on the bottom label printer (Printer 4).
Detail | The label is not issued in time. The label may be jammed.
Solution | Touch [OK] button.
Action by user | Make sure that the label is not jammed.
Action by service representative | In the past, there was a case where a problem occurred when the auto-attach label length was changed from the default 105 mm to 200 mm and a 110 mm label was continuously and automatically attached. Select “Adjust Mode" and "Printer", then select “Under” on the "Label Feed" tab screen to display the setting item “Auto Paste Label Length”.
Related part | Bottom label printer board
Remarks | Bottom label printer (Printer 4) dedicated error