- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Product is remaining inside of infeeder (514)

Error content | The product remains in the automatic infeeder.
Detail | This error occurs when a product is left on the conveyor at the start of the empty PS-AI and while the conveyor is being driven. The sub-error has the following meanings: 0001: The product was detected by the feed bar ON sensor in the pre-operation check. 0002: The product was detected by the tray stop sensor in the pre-operation check. 0011: The remaining product was detected by the feed bar ON sensor or tray stop sensor immediately after the conveyor started. 0100: The product is stuck at the tray separation sensor (front) during transportation.
Release method | Open the cover, remove the product, and press the [RETURN] button.
User’s action | Open the cover, remove the product, and press the [RETURN] button.
Service action |
Relevant locations | 1) P-1105[A600] 2) Tray stop sensor [B606] 3) Feed bar ON sensor [B605] 4) Tray separation sensor (front) [B604]
Remarks |