< Motor front feeder move is abnormal (419)

Error content | Motor front feeder error.
Detail | Motor front feeder operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 P-1006 board for front feeder [A201] 嘊 Driving motor for feeder [M09] 嘋 Origin point of front feeder [B***]
Remarks |