< Outfeed pusher motor is abnormal (417)

Error content | Outfeed pusher motor error.
Detail | Outfeed pusher motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0002: Cannot detect speed pulse signal from the DCB motor (driver board). 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0005: Began next product operation before the previous operation was completed (unsuitable wrapper condition). 0006: The next product stuck out before the previous operation was completed (unsuitable wrapper condition). 1003: Tray press operation wasn乫t completed when the operation protection timer run out.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A100] 嘇 Driving motor for outfeed pusher [M01]
Remarks |