< There is problem on wrapping controller (472)

Error content | Wrapper wiring board error.
Detail | A communication error occurred between parent (wrapper control board: P-1105: A200) and child (P-1105: A100, A300). Sub-error meanings are as follows: 0000: A communication error between P-1105 [A100] and P-1105 [A300]. 0001: A communication error with P-1105 [A300]. 0002: A communication error with P-1105 [A100].
Solution | Restore power
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A100], [A200], [A300] 嘇 23-pin and 24-pin in XJ7 of P1105 [A100] must be short-circuited. 嘊 21-pin and 22-pin in XJ7 of P1105 [A200] must be short-circuited. 嘋 21-pin and 22-pin, and 23-pin and 24-pin in XJ7 of P1105 [A100] must be short-circuited.
Remarks |