n Thermal head for under labeller is up (1016-0002)

Error content | Thermal head for the under labeller is up.
Detail | The thermal head was up when printing starts. Displaying when closing the front cover or setting the under labeller unit.
Solution | Pull the under labeller unit out, press [RETURN] button after setting the thermal head.
Action by user |
Action by service representative |
Related part |
Remarks |