< Left film exchange cover is open (0309)

Error content | Left film exchange cover is open.
Detail | Occurs when the left film exchange cover is open before operation.
Solution | Close left film exchange cover, [OK] button.
Action by user | Close the film replacement door on the left.
Action by service representative | Close the film replacement door on the left.
Related part | Main board, wrapping machine board
Remarks |