< Insert plate is not set for the upper (478)

Error content | Insert plate is not set for the upper.
Detail | Film exchange cover is closed, but upper film 丂 insert open/close is open.
Solution | Press the [RETURN] button after setting the insert plate.
Action by user |
Action by service representative |
Related part | <If the error persists even after the insert open/close is closed> 嘆 P-1105 [A300] 嘇 Upper film inserts open/close [B307].
Remarks |