< Blackout for the console (604)

Error content | Power failure detected in the applicator.
Detail | Power ON notification command was received twice from the console.
Solution | Restore power
Action by user |
Action by service representative |
Related part | 嘆 24 V DC to the power supply (XJ12) of P-1105 [A100]. 嘇 RS485 communication cable between main boards (P-1100, P-1163, P-1000) [A10] and P-1105 [A100].
Remarks |