< No response from tray detector (1502)

Error content | No response from tray detector.
Detail | Unable to communicate between the console and the tray detector. The communication phase number is in the sub-error. Errors after power ON process completion result in this error.
Solution | [STOP] button => Cut communication with the detector. Operate without the detector. [REEXEC] button => Check connection with the detector. If connection can be confirmed, the error is cleared.
Action by user |
Action by service representative | Confirm the RS485 communication line of the main board (P-1100, P-1163, P-1000). Confirm RS485 communication line [A221 XJ-11] and 24VDC power supply [A221 XJ-9] of the detector board.
Related part | Main board (P-1100, P-1163, P-1000) [A10] Detector board (P-1107) [A221]
Remarks |