- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Wrapper detected temporary blackout (406)

Error content | The wrapper control board detected the CPU reset.
Detail | The console received power ON notification (status query) twice from the wrapper.
Solution | Restore power
Action by user | Perform a power cycle.
Action by service representative |
Related part | ① P-1105 [A200] ② Control unit section switching power supply [U10]
Remarks |