< Lift motor is abnormal (410)

Error content | Lift motor is abnormal
Detail | Lift motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn't completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0101: The lower side of lift [B203] is not receiving light, when lowering the lift. 0102: The lower side of lift [B203] is emitted light, after switching or returning the lift. 0103: The origin point of lift [B202] and the lift safety [B204] are not receiving light. when the lift backs to its origin point. 0104: The origin point of lift [B202] and the lift safety [B204] are not receiving light when the lift is in its switch position. 0105: The origin point of lift [B202] is not receiving light when lowering the lift. The lift lower side position [B203] is emitted light wen the lift backs to its origin point. 0106: Do not block light of the lift origin point [B200] when the lift is moving to the origin point after the lift changeover. 0107: The lift origin point [B200] is not receiving light when lowering the lift. 0201: The lift origin point [B200] is not receiving light even after a certain period of time after the lift starts operation.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Motor for lift [M06] 嘊 Sensors described above: [B200], [B202], [B203], [B204]
Remarks |