- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Product is on the lift (486)

Error content | Product is on the lift
Detail | There was a product on the lift when each of the following operations was started (completed). Sub-error meanings are as follows: 0000: After completion of returning operation. 0004: Wrapping the first product is attempted. 0007: Shifting to sleep mode. Others: Sending film or film loading is attempted.
Solution | Press the [RETURN] button after removing the product.
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Detection of products on the lift [B206].
Remarks |