< Motor voltage is abnormal (435)

Error content | Power supply voltage error.
Detail | Occurs when voltage error is detected in the P-1105 board. Sub-error meanings are as follows: 0001: Undervoltage was detected in P-1105 [A200]. 0002: Overvoltage was detected in P-1105[A200]. 0011: Undervoltage was detected in P-1105 [A100]. 0012: Overvoltage was detected in P-1105 [A100]. 0021: Undervoltage was detected in P-1105 [A300]. 0022: Overvoltage was detected in P-1105 [A300].
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 Confirm the power supply of input power 200 to 240 V AC. 嘇 P-1105 [A100, A200, A300]
Remarks |