- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Automatic label length adjustment (1861-1000)

Error content | Displayed pressing [AUTO LNG. ADJUST] button on LABEL APPLICATOR (LABEL) screen.
Detail | Confirm to execute the automatic label length adjustment.
Solution | Press [EXEC] or [STOP] button. [EXEC]: Head check is performed to the next product. [STOP]: Head check is not performed to the next product.
Action by user | Press [EXEC] or [STOP] button.
Action by service representative
Related part |
Remarks | Only for POP printer.