- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film heater has problem (426)

Error content | Film heater error.
Detail | As an error occurs in film heater, unable to use the heater. Sub-error meanings are as follows: 0001: Thermistor of film heater is disconnected. 0100: A fan alarm occurs (alarm also occurs when connector is not inserted).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A300] ② Thermistor for film heater [R300] ③ Fan for film heater [M305]: Sub-error is 100
Remarks | After the error occurrence, unable to use the left side film heater.