< Motor for film feed is abnormal (411)

Error content | Motor for film feed is abnormal.
Detail | Film insert motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0011: The insert motor was stepped out when the film is traveling. 0021: The insert didn乫t back to the normal position when the cutter starts operation.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A300] 嘇 P-1006 [A301] 嘊 Stepping motor for film feed [M303] 嘋 Film feed origin point [B301]
Remarks |