< A uxiliary for magnetic contact is abnormal (485)

Error content | Auxiliary for magnetic contact is abnormal
Detail | Error occurred between the electromagnetic contact auxiliary contact input opening and closing the power line and each cover switch open/closed condition while waiting for the wrapper or during operation. This electromagnetic switch is blocking the power line (200VAC, 24VDC). For example, if the electromagnetic switch auxiliary contact is open and each cover safety switch and the emergency stop switch are closed and this error continues for 5 seconds, this error occurs. The switch location where the error occurred is displayed in the sub-error as below. If multiple covers are open, values given below are added and displayed in the sub-error. 2048: Film replacement cover open. 1024: Front cover is open. 0256: Infeed conveyors pulled out. 0128: Emergency stop switch ON. 0064: Film removal cover is open. 0000: No cover is open.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | [485-0000] 嘆 P-1105 [A100-XJ19] 嘇 Magnetic contact [K100, K101] and wiring of magnetic contact. [Other than 485-0000] 嘆 Wiring to the switch described in the detail.
Remarks | It is not an actual failure; however, this error occurs easily when a cover is half-way closed.