- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Outfeed pusher motor is abnormal (417)

Error content | Outfeed pusher motor error.
Detail | Outfeed pusher motor operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn’t completed when the operation protection timer run out. 0002: Cannot detect speed pulse signal from the DCB motor (driver board). 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0005: Began next product operation before the previous operation was completed (unsuitable wrapper condition). 0006: The next product stuck out before the previous operation was completed (unsuitable wrapper condition). 1003: Tray press operation wasn’t completed when the operation protection timer run out.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A100] ② Driving motor for outfeed pusher [M01]
Remarks |