- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Cannot connect with camera unit (1506)

Error content | Unable to communicate between tray detector and the tray detector camera.
Detail | It has been decided that the camera is not connected due to the inability to obtain a proper response when attempting to set the camera.
Solution | [OK] button => Operate without the tray detector. (Operate with registered trays.)
Action by user |
Action by service representative | Confirm the connection between the detector board and CMOS camera [A221 XJ-4].
Related part | Detector board (P-1107) [A221] CMOS camera
Remarks |