- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■ It could not suck label (00609)

Error content | Applicator failed in label application.
Detail | Sub-error meanings are as follows: 0000: Applicator failed in labeled absorption.
Solution | Use either (1) or (2) to clear the error. ① [RETURN] button ② [PLU] button
Action by user | Clean up the label presence sensor.
Action by service representative | Clean up the label presence sensor. Adjust the issue position by printing adjustment. Adjust the suction position on the printer adjustment screen.
Related part | ① P-1105 [A100] ② P-1006 [A101] ③ Label presence [B116] ④ Label suction fan [M107]
Remarks | ■Past example 1 Symptom: The label format or label sizing was changed, causing an error when the label applicator sucked the label. Cause: Judged that there was no label because the black printed part of the label and the label presence sensor [B116] matched the position and the label presence sensor was dirty. Handling: Cleaned the label presence sensor [B116]. ■Past example 2 Symptom: An error was displayed before the label applicator went to pick up the label and pasted it on the product. Cause: Judged that there was no label in the middle of the label applicator's movement due to the dirt on the label presence sensor. Handling: Cleaned the label presence sensor [B116].