- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Label is remaining (0312)

0312-0000 | The label remains.
0312-0000 | The label remains on the POP label printer (Printer 5).
0312-0001 | The label remains on the label sticking part. Blinking green LED: Label applicator Blinking yellow LED: Printer
0312-0002 | The label remains on the POP label sticking part.
0312-0004 | The label remains on the bottom label printer (Printer 4).
0312-0005 | The label remains on the label sticking part of the bottom label printer (Printer 4).

Error content | The peel sensor or label suction sensor detected the remaining label when the label was issued. Checking the same sensor as in the case of error 0351.
Detail | The sub-error number tells you where the problem is. 0000: Peeling sensor In the pre-check before printing starts, the peeling sensor is in a light-shielded state (the peeling sensor value is below the threshold value). The peel sensor may be dirty, so clean the sensor. Adjust the sensitivity of the peeling sensor. It is important that the optical axis of the sensor is aligned. 0001: Label applicator The label detection sensor is in a reflective state and the label remains on the label applicator. This can be confirmed on the sensor check screen of the top label applicator. 0002: POP label applicator The label detection sensor is in a reflective state and the label remains on the label applicator. This can be confirmed on the sensor check screen of the top label applicator. 0004: Bottom label printer Remove the label on the roller of the bottom label printer.
Solution | RRemove the label on the printer and press the [OK] button.
User’s action | Remove the label on the printer and take the slack out of the label mount. Remove the label on the label applicator.
Service person’s action | Check the operation of the peeling sensor of the printer in which the error has occurred. Check the label detection sensor of the label applicator (top label applicator sensor check). Failure signal from XJ6 on the P-1163 [A10] board (board failure)
Related part | Printer 1: Main board P-1163, Peeling sensor Printer 2: Printer board P-1001, Peeling sensor Label applicator: Wrapping board P-1105 [A100] (upper left) XJ-20, P-1006-5 (A101) XJ-5 and 7, label detection sensor, curl cord, movable harness POP label applicator: Wrapping board P-1105 [A100] (upper right) XJ-20, P-1006-5 (A401) XJ-5 and 7, label detection sensor, curl cord, movable harness
Remarks | Error 0312: This error occurs when the label was detected in the pre-check for operation Error 0351: Error that occurs when the remaining label error display time is set.