- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Cutter original position error (1088-0000)

Error content | Cutter original position error.
Detail | Cutter is not located at original position.
Solution | Press [EXEC] button to operate a cutter.
Action by user |
Action by service representative |
Related part |
Remarks |