< Abnormal for applicator (615)

Error content | Abnormal for applicator.
Detail | Operation was not completed within the set time. Sub-error meanings are as follows: 000*: X axis (* = 0: moving left, 1: moving right) 001*: Y axis (* = 0: moving forward, 1: moving backward) 002*: Z axis (* = 0: moving up, 1: moving down) 003*: 兤 axis (* = 0: rotating to right, 1: rotating to left) 013*: 兤 axis (* = 0: rotating to right, 1: rotating to left) In case that a sensor event does not occur after the set time, while operating corrections. 0100: Absorption was expected to be done by printer No.1, however, the applicator was moved in front of printer No.2. 0101: Absorption was expected to be done by printer No.2, however, the applicator was moved in front of printer No.1.
Solution | [RETURN] button
Action by user | Check if the printer can be moved smoothly with hands with the emergency stop switched pressed.
Action by service representative | Check the grease condition.
Related part | <X axis> 嘆 P-1105 [A100] 嘇 P-1006 [A102] 嘊 X-axis motor [M103] 嘋 X-axis origin point [B108] 嘍 Printer No.1 position [B109] 嘐 Printer No.2 position [B110] <Y axis> 嘆 P-1105 [A100] 嘇 P-1006 [A101] 嘊 Y-axis motor [M104] 嘋 Y-axis origin point [B111] <Z axis> 嘆 P-1105 [A100] 嘇 P-1006 [A101], [A102] 嘊 Z-axis motor [M105] 嘋 Z-axis origin point [B112] <q axis> 嘆 P-1105 [A100] 嘇 P-1006 [A101] 嘊 q-axis motor [M106] 嘋 Below q-axis detection board [B113] 嘍 Above q-axis detection board [B114]
Remarks |