< Film loading instructions (597 亅 0000)

Error content | Film loading instructions.
Detail | Message indicates that the insert plate reached the film set position. Sets the film size or film. [UPPER FILM] sets the upper film size.
Solution | 嘆 Press either the [RETURN] button or the [SET FILM] button. [RETURN]: Returns to the original screen. *Film size returns to the original data. [SET FILM]: Sets the film. 嘇 Open the film exchange cover and close the cover after the film is set.
Action by user |
Action by service representative |
Related part |
Remarks | Sub-error 0000 is displayed when upper film is set.