< There is problem on seal heater (474)

Error content | Back outfeed heater error.
Detail | An error occurred in either the rear heater or the thermostat monitoring the rear heater temperature. Sub-error meanings are as follows: 0000: The heater temperature does not rise while heating (Thermostat value does not change). 0001: Thermostat error (Disconnection or short circuit).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Outfeed front heater [E71]. 嘊 Fuse for outfeed heater [F106, F107]. 嘋 Thermistor for outfeed front heater [R2]. 嘍 SSR for outfeed front heater [K201].
Remarks | The heater is switched OFF when this error occurs.