- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< No response from wrapper (402)

Error content | There was no response with respect to the inquiry conducted by the main board(P-1000/P-1100/P-1163) to the wrapper board P-1105 [A200] about the state. During communication retrial, a beep error sound is heard for "20 times", indicating that retrials are in progress. If communication is not established, an error is displayed.
Detail | This is a communication error that has occurred after performing power-on processing. The sub-error includes the communication phase number. When no communication is possible due to a board defect or disconnection of wire harness, the sub error will become "0000". 0000： Communication is not established at the initial stage of communication
Solution | Press [STOP] to release the error. Press [REEXEC] to check the connection with the wrapper again.
User’s action | Turn off the power supply and then turn on the power supply again. By pressing the [STOP] button on the error display screen, the wrapper can be disconnected and used as a pricing printer.
Service person’s action | Check RS-485 communication line (harness disconnection, connector contact failure) Between P-1105 [A100] (XJ27) and P-1105 [A300] (XJ26) Between P-1105 [A300] (XJ27) and P-1105 [A200] (XJ27) Defective RS-485 communication port on P-1105 [A100, A200, A300] When the RS-485 communication port on the main board (P-1000, P-1100, P-1163) [A10] is defective, 1502-0000 (No response from tray detector) is also be displayed.
Related part | ①P-1105 [A100] XJ26, XJ27 ②P-1105 [A200] XJ26, XJ27 ③P-1105 [A300] XJ27 ②DC 24V supply to the power supply (XJ12) of P-1105 [A100], [A200], [A300] (DC 24V is normally supplied when the LED of P-1105 [A200] is lit.) ③RS485 communication cable between P-1105 [A100, A200, A300] The following RS485 communication has not been established: Between P-1000/P-1100/P-1163 [A10] (XJ4) and P-1105 [A100] (XJ26) Between P-1105 [A100] (XJ27) and P-1105 [A300] (XJ26) Between P-1105 [A300] (XJ27) and P-1105 [A200] (XJ27)
Remarks | Pricing is only possible after the [STOP] button is pressed.

Click to open PDF file