- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n POP applicator has stopped (608-2000)

Error content | Applicator has stopped.
Detail | The emergency stop switch was used during POP applicator is operating.
Solution | Press [RETURN] button.
Action by user | Press [RETURN] button.
Action by service representative
Related part |
Remarks |