< Wrapper is not connected (401)

Error content | Wrapper is not connected.
Detail | Communication error before power has been turned ON. Communication phase No. is listed in the sub-error.
Solution | [STOP] button 亖> Cancel error [REEXEC] button => Re-check the connection with the wrapper.
Action by user | Perform turn ON/OFF of the power supply.
Action by service representative |
Related part |
Remarks | After pressing the [STOP] button, only pricing can be performed.