- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Do not put your hands into the machine (449)

Error content | A hand was put into the wrapper during operation.
Detail | Occurs when a hand or object is detected entering the infeed conveyor while the wrapper is operating. Sub-error meanings are as follows: 0000: Detected by a sensor located over the outfeed heater. 0001: Detected by a sensor located under the cover.
Solution | Press the [RETURN] button after making sure a hand or object is not placed.
Action by user |
Action by service representative |
Related part | ① P-1105 [A100] ② Hand insertion in the outfeeder (light receiving/emitting) [B106]: Sub-error is 0000. ③ Hand insertion in the front cover (light receiving/emitting) [B107]: Sub-error is 0001.
Remarks |