- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film is remaining (480－0101)

Error content | Film is remaining.
Detail | The film sensor board is knocked over when the film started to be sent. The bit mask shows the knocked over sensor location. Number and location correlation are as follows: 0001: Rear right 0010: Front right 0100: Rear left 1000: Front left (Ex) If remaining film were detected in the rear right and front right, the sub-error would be 0011.
Solution | Press the [RETURN] button after removing film.
Action by user |
Action by service representative |
Related part | <If the error occurs even after the film is removed> ① P-1105 [A200] ② Film presence front right [B209]. ③ Film presence front left [B208]. ④ Film presence rear left [B210]. ⑤ Film presence rear right [B211].
Remarks |