< Problem on tray detector (1503)

Error content | The command sent to the applicator and the command contained in the answer is different.
Detail |
Solution | Restore power
Action by user |
Action by service representative | Confirm the RS485 communication line of the main board (P-1100, P-1163, P-1000). Confirm RS485 communication line [A221 XJ-11] and 24 V DC power supply [A221 XJ-9] of the detector board.
Related part | Main board (P-1100, P-1163, P-1000) [A10] Detector board (P-1107) [A221]
Remarks |