- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■ POP printer cover is not set (01967-0000)

Error content | POP label cover is opening.
Detail | Occurs when the cover open starting operation.
Solution | Touch [OK] button.
Action by user | Close the label cover and touch [OK] button.
Action by service representative | Close the label cover and touch [OK] button. Conform the label cover sensor.
Related part | Label cover sensor
Remarks | Only for POP printer.