< Right film remove cover is open (0306)

Error content | Right film remove cover is open.
Detail | Occurs when the right film remove cover is open before operation.
Solution | Close Right film remove cover, [OK] button.
Action by user | Close the film removal door on the right.
Action by service representative | Close the film removal door on the right.
Related part | Main board, wrapping machine board
Remarks |