< Motor rear feeder move is abnormal (420)

Error content | Motor rear feeder error.
Detail | Motor rear feeder operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn乫t completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 Driving motor for feeder [M09] 嘊 Origin point of rear feeder [B212]
Remarks |