< No response from wrapper (402)

Error content | No response from wrapper.
Detail | Communication error after power has been turned ON. Communication phase is listed in the sub-error.
Solution | [STOP] button => Cancel error. [REEXEC] button => Re-check the connection with the wrapper.
Action by user | Perform a power cycle.
Action by service representative |
Related part | 嘆 P-1105 [A200] 嘇 24VDC to the power supply (XJ12) of P-1105 [A200] 嘊 RS485 communication cable between main boards (P-1100, P-1163, P-1000) [A10] and P-1105 [A100, A200, A300]
Remarks | After pressing the [STOP] button, only pricing can be performed.